
  
3. Supporting the remote control button operation instructions
[image: 2825b66f0d9056a7e2dbb71e5dc4b85]ON/OFF: on/off
Strobe: strobe
DMX:A001 menu
Auto: Self-propelled mode 1
MENU: menu plus
Jump: Self-propelled mode 28
Falsh: self-propelled mode 30
Sound:SU01-voice control
Add numerical value: ↑
Numerical subtraction: ↓
RED: w1
GREEN：w2
BLUE：w3
AMBER：w1w2
CYAN: w2w3
ROSEO: w1w3
WHITE：w1w2w3














9-pcs golden light instructions
I. The DMX channel menu

11 Channel (Basic Function)
	channel
	value
	function declaration

	CH 1
	000-255
	Total dimming, from dark to bright

	CH 2
	005-255
	Total strobe, from slow to fast

	CH 3
	000-004
	Perform the (CH 9-11) RGB static dimming

	
	005-009
	Static color, CH4 Select (WHITE1,WHITE2,WHITE3)

	
	010-014
	Breathing effect, CH5 Select color

	
	015-019
	Jump change effect, CH5 Select color

	
	020-024
	Gradient change effect, (full color effect)

	
	025-029
	Pulse change effect, CH5 Select color

	
	030-037
	[bookmark: OLE_LINK3]Autorun effect-1, CH5 Select color(cycle autorun)

	
	038-045
	Autorun effect-2, CH5 Select color

	
	046-053
	Autorun effect-3, CH5 Select color

	
	...
	...

	
	...
	...

	
	214-221
	Autorun effect-24, CH5 Select color

	
	222-229
	Autorun effect-25, (full color effect)

	
	230-239
	Autorun effect-26, (full color effect)

	
	240-244
	Sound mode 1, CH5 Select color

	
	245-249
	Sound mode 2, CH5 Select color

	
	250-255
	Sound mode 3, CH5 Select color

	CH 4
	000-255
	Static color mode: WHITE1,WHITE2,WHITE3
Autorun effect: adjustment speed, from slow to fast .
Sound mode: adjustment sensitivity, from low to high (The highest sensitivity is the sensitivity set by the menu) .

	CH 5
	000-028
	Default color

	
	029-056
	Red, CH3 Manual color selection

	
	057-085
	Green, CH3 Manual color selection

	
	086-113
	Blue, CH3 Manual color selection

	
	114-142
	Yellow, CH3 Manual color selection

	
	143-170
	Purple, CH3 Manual color selection

	
	171-199
	Cyan, CH3 Manual color selection

	
	200-227
	White, CH3 Manual color selection

	
	228-255
	User-defined color(CH6-CH8), CH3 Manual color selection

	CH 6
	000-255
	Autorun effect color: WHITE1 dimming, from dark to bright

	CH 7
	000-255
	Autorun effect color: WHITE2 dimming, from dark to bright

	CH 8
	000-255
	Autorun effect color: WHITE3 dimming, from dark to bright

	CH 9
	000-255
	Background color: WHITE1 dimming, from dark to bright

	CH 10
	000-255
	Background color: WHITE2 dimming, from dark to bright

	CH 11
	000-255
	Background color: WHITE3 dimming, from dark to bright



3 Channel (whole lamp)
	channel
	value
	function declaration

	CH 1
	000-255
	WHITE1 dimming, from dark to bright

	CH 2
	000-255
	WHITE2 dimming, from dark to bright

	CH 3
	000-255
	WHITE3 dimming, from dark to bright



5 Channel (whole lamp)
	channel
	value
	function declaration

	CH1
	000-255
	Total dimming, from dark to bright

	CH 2
	005-255
	Total strobe, from slow to fast

	CH 3
	000-255
	WHITE1 dimming, from dark to bright

	CH 4
	000-255
	WHITE2 dimming, from dark to bright

	CH 5
	000-255
	WHITE3 dimming, from dark to bright



108 Channel (point control)
	channel
	value
	function declaration

	CH 1
	000-255
	WHITE1-1 dimming, from dark to bright

	CH 2
	000-255
	WHITE2-1 dimming, from dark to bright

	CH 3
	000-255
	WHITE3-1 dimming, from dark to bright

	...
	...
	...

	...
	...
	...

	CH 106
	000-255
	WHITE1-36 dimming, from dark to bright

	CH 107
	000-255
	WHITE2-36 dimming, from dark to bright

	CH 108
	000-255
	WHITE3-36 dimming, from dark to bright





110 Channel (point control)
	channel
	value
	function declaration

	CH1
	000-255
	Total dimming, from dark to bright

	CH 2
	005-255
	Total strobe, from slow to fast

	CH 3
	000-255
	WHITE1-1 dimming, from dark to bright

	CH 4
	000-255
	WHITE2-1 dimming, from dark to bright

	CH 5
	000-255
	WHITE3-1 dimming, from dark to bright

	...
	...
	...

	CH 108
	000-255
	WHITE1-36 dimming, from dark to bright

	CH 109
	000-255
	WHITE2-36 dimming, from dark to bright

	CH 110
	000-255
	WHITE3-36 dimming, from dark to bright



II. Key operation and digital tube display instructions
1. Key description

[bookmark: _GoBack][image: ]
MENU: function key	UP: Key+ DOWN: key- ENTER: Confirm key
2. Digital tube display menu description
	number
	content
	value
	function declaration

	1
	A001
	001 - 512
	The DMX512 address setting

	2
	11CH
	3/5/11/108/110
	Channel mode setting

	3
	R255
	000 - 255
	WHITE1 dimming, from dark to bright

	4
	G255
	000 - 255
	WHITE2 dimming, from dark to bright

	5
	B255
	000 - 255
	WHITE3 dimming, from dark to bright

	6
	F000
	005 - 255
	Total strobe, from slow to fast

	7
	CL01
	01 - 07
	red, green, blue, yellow, purple, cyan, white

	8
	EF01
	01 - 30
	UP to switch the effect
	Press ENTER to set the speed SP01-SP15

	9
	SU01
	01 - 03
	Sound mode
	Press ENTER to set the sensitivity SE01-SE15
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